McPAT (version 0.8 of Aug, 2010) is computing the target processor...
 

McPAT (version 0.8 of Aug, 2010) results  (current print level is 5)
*****************************************************************************************
  Technology 40 nm
  Interconnect metal projection = conservative interconnect technology projection
  Target Clock Rate (MHz) 1700

*****************************************************************************************
  System:
    Area = 10.8081 mm^2
    Peak Dynamic Power = 2.45616 W
    Subthreshold Leakage Power = 4.64481 W
    Gate Leakage Power = 0.193831 W
    Runtime Dynamic Power = 1.32073 W
    Runtime Dynamic Energy = 1.16535e-07 J
    Total Runtime Energy = 5.43474e-07 J

      Core 0:
        Area = 10.8081 mm^2
        Peak Dynamic Power = 2.45616 W
        Subthreshold Leakage Power = 4.64481 W
        Gate Leakage Power = 0.193831 W
        Runtime Dynamic Power = 1.32073 W
        Runtime Dynamic Energy = 1.16535e-07 J
        Total Runtime Energy = 5.43474e-07 J

          Instruction Fetch Unit:
            Area = 2.10081 mm^2
            Peak Dynamic Power = 0.33569 W
            Subthreshold Leakage Power = 0.347428 W
            Gate Leakage Power = 0.00868165 W
            Runtime Dynamic Power = 0.213414 W
            Runtime Dynamic Energy = 1.88306e-08 J
            Total Runtime Energy = 5.0252e-08 J

              Instruction Cache:
                Area = 0.970326 mm^2
                Peak Dynamic Power = 0.0549304 W
                Subthreshold Leakage Power = 0.0678485 W
                Gate Leakage Power = 0.00157419 W
                Runtime Dynamic Power = 0.0505595 W
                Runtime Dynamic Energy = 4.46113e-09 J
                Total Runtime Energy = 1.05867e-08 J

                  Data and Tag Arrays:
                    Area = 0.25887 mm^2
                    Peak Dynamic Power = 0 W
                    Subthreshold Leakage Power = 0.0622886 W
                    Gate Leakage Power = 0.00129234 W
                    Runtime Dynamic Power = 0.0464002 W
                    Runtime Dynamic Energy = 4.09413e-09 J
                    Total Runtime Energy = 9.70422e-09 J

                  Miss Buffer:
                    Area = 0.262959 mm^2
                    Peak Dynamic Power = 0.0192867 W
                    Subthreshold Leakage Power = 0.00194663 W
                    Gate Leakage Power = 9.86469e-05 W
                    Runtime Dynamic Power = 0.00146456 W
                    Runtime Dynamic Energy = 1.29226e-10 J
                    Total Runtime Energy = 3.09692e-10 J

                  Fill Buffer:
                    Area = 0.224249 mm^2
                    Peak Dynamic Power = 0.0178218 W
                    Subthreshold Leakage Power = 0.00180662 W
                    Gate Leakage Power = 9.16038e-05 W
                    Runtime Dynamic Power = 0.00134737 W
                    Runtime Dynamic Energy = 1.18886e-10 J
                    Total Runtime Energy = 2.86376e-10 J

                  Prefetch Buffer:
                    Area = 0.224249 mm^2
                    Peak Dynamic Power = 0.0178218 W
                    Subthreshold Leakage Power = 0.00180662 W
                    Gate Leakage Power = 9.16038e-05 W
                    Runtime Dynamic Power = 0.00134737 W
                    Runtime Dynamic Energy = 1.18886e-10 J
                    Total Runtime Energy = 2.86376e-10 J

              Branch Target Buffer:
                Area = 0.526552 mm^2
                Peak Dynamic Power = 0.0433889 W
                Subthreshold Leakage Power = 0.0869885 W
                Gate Leakage Power = 0.00266245 W
                Runtime Dynamic Power = 0.0189877 W
                Runtime Dynamic Energy = 1.67538e-09 J
                Total Runtime Energy = 9.58576e-09 J

              Branch Predictor:
                Area = 0.594319 mm^2
                Peak Dynamic Power = 0 W
                Subthreshold Leakage Power = 0.186556 W
                Gate Leakage Power = 0.00424723 W
                Runtime Dynamic Power = 0.0647432 W
                Runtime Dynamic Energy = 5.71264e-09 J
                Total Runtime Energy = 2.25483e-08 J

                  Global Predictor:
                    Area = 0.129022 mm^2
                    Peak Dynamic Power = 0 W
                    Subthreshold Leakage Power = 0.0419609 W
                    Gate Leakage Power = 0.000962899 W
                    Runtime Dynamic Power = 0.0172467 W
                    Runtime Dynamic Energy = 1.52177e-09 J
                    Total Runtime Energy = 5.30916e-09 J

                  Local Predictor, Level 1:
                    Area = 0.191924 mm^2
                    Peak Dynamic Power = 0 W
                    Subthreshold Leakage Power = 0.0589594 W
                    Gate Leakage Power = 0.00130932 W
                    Runtime Dynamic Power = 0.0255552 W
                    Runtime Dynamic Energy = 2.25487e-09 J
                    Total Runtime Energy = 7.5727e-09 J

                  Local Predictor, Level 2:
                    Area = 0.129022 mm^2
                    Peak Dynamic Power = 0 W
                    Subthreshold Leakage Power = 0.0419609 W
                    Gate Leakage Power = 0.000962899 W
                    Runtime Dynamic Power = 0.0046946 W
                    Runtime Dynamic Energy = 4.1423e-10 J
                    Total Runtime Energy = 4.20162e-09 J

                  Predictor Chooser:
                    Area = 0.129022 mm^2
                    Peak Dynamic Power = 0 W
                    Subthreshold Leakage Power = 0.0419609 W
                    Gate Leakage Power = 0.000962899 W
                    Runtime Dynamic Power = 0.0172467 W
                    Runtime Dynamic Energy = 1.52177e-09 J
                    Total Runtime Energy = 5.30916e-09 J

                  RAS:
                    Area = 0.0153301 mm^2
                    Peak Dynamic Power = 0 W
                    Subthreshold Leakage Power = 0.0017144 W
                    Gate Leakage Power = 4.92127e-05 W
                    Runtime Dynamic Power = 0 W
                    Runtime Dynamic Energy = 0 J
                    Total Runtime Energy = 1.55613e-10 J

              Instruction Buffer:
                Area = 0.0034347 mm^2
                Peak Dynamic Power = 0.011729 W
                Subthreshold Leakage Power = 0.000650517 W
                Gate Leakage Power = 1.85414e-05 W
                Runtime Dynamic Power = 0.00390968 W
                Runtime Dynamic Energy = 3.44972e-10 J
                Total Runtime Energy = 4.04006e-10 J

              Instruction Opcode Decoder:
                Area = 0.00289896 mm^2
                Peak Dynamic Power = 0.0752588 W
                Subthreshold Leakage Power = 0.00253168 W
                Gate Leakage Power = 8.37387e-05 W
                Runtime Dynamic Power = 0.0250863 W
                Runtime Dynamic Energy = 2.2135e-09 J
                Total Runtime Energy = 2.44427e-09 J

              Instruction Operand Decoder:
                Area = 0.000377341 mm^2
                Peak Dynamic Power = 0.0751236 W
                Subthreshold Leakage Power = 0.00032028 W
                Gate Leakage Power = 1.17596e-05 W
                Runtime Dynamic Power = 0.0250412 W
                Runtime Dynamic Energy = 2.20952e-09 J
                Total Runtime Energy = 2.23881e-09 J

              Instruction Microcode Decoder:
                Area = 0.00289896 mm^2
                Peak Dynamic Power = 0.0752588 W
                Subthreshold Leakage Power = 0.00253168 W
                Gate Leakage Power = 8.37387e-05 W
                Runtime Dynamic Power = 0.0250863 W
                Runtime Dynamic Energy = 2.2135e-09 J
                Total Runtime Energy = 2.44427e-09 J

          Load/Store Unit:
            Area = 1.69899 mm^2
            Peak Dynamic Power = 0.16674 W
            Subthreshold Leakage Power = 0.0926715 W
            Gate Leakage Power = 0.00259372 W
            Runtime Dynamic Power = 0.142557 W
            Runtime Dynamic Energy = 1.25786e-08 J
            Total Runtime Energy = 2.09843e-08 J

              Data Cache:
                Area = 1.58391 mm^2
                Peak Dynamic Power = 0.0928926 W
                Subthreshold Leakage Power = 0.0789233 W
                Gate Leakage Power = 0.00207502 W
                Runtime Dynamic Power = 0.0922726 W
                Runtime Dynamic Energy = 8.1417e-09 J
                Total Runtime Energy = 1.52886e-08 J

                  Data and Tag Arrays:
                    Area = 0.619642 mm^2
                    Peak Dynamic Power = 0 W
                    Subthreshold Leakage Power = 0.0607406 W
                    Gate Leakage Power = 0.00122316 W
                    Runtime Dynamic Power = 0.0861866 W
                    Runtime Dynamic Energy = 7.6047e-09 J
                    Total Runtime Energy = 1.30721e-08 J

                  Miss Buffer:
                    Area = 0.270528 mm^2
                    Peak Dynamic Power = 0.0245073 W
                    Subthreshold Leakage Power = 0.0048041 W
                    Gate Leakage Power = 0.000224896 W
                    Runtime Dynamic Power = 0.00214283 W
                    Runtime Dynamic Energy = 1.89073e-10 J
                    Total Runtime Energy = 6.32808e-10 J

                  Fill Buffer:
                    Area = 0.231248 mm^2
                    Peak Dynamic Power = 0.0227951 W
                    Subthreshold Leakage Power = 0.00445956 W
                    Gate Leakage Power = 0.000208987 W
                    Runtime Dynamic Power = 0.00197161 W
                    Runtime Dynamic Energy = 1.73965e-10 J
                    Total Runtime Energy = 5.85896e-10 J

                  Prefetch Buffer:
                    Area = 0.231248 mm^2
                    Peak Dynamic Power = 0.0227951 W
                    Subthreshold Leakage Power = 0.00445956 W
                    Gate Leakage Power = 0.000208987 W
                    Runtime Dynamic Power = 0.00157729 W
                    Runtime Dynamic Energy = 1.39172e-10 J
                    Total Runtime Energy = 5.51103e-10 J

                  Writeback Buffer:
                    Area = 0.231248 mm^2
                    Peak Dynamic Power = 0.0227951 W
                    Subthreshold Leakage Power = 0.00445956 W
                    Gate Leakage Power = 0.000208987 W
                    Runtime Dynamic Power = 0.000394322 W
                    Runtime Dynamic Energy = 3.47931e-11 J
                    Total Runtime Energy = 4.46724e-10 J

              Load Queue:
                Area = 0.054217 mm^2
                Peak Dynamic Power = 0.0316525 W
                Subthreshold Leakage Power = 0.00559768 W
                Gate Leakage Power = 0.00022125 W
                Runtime Dynamic Power = 0.0137161 W
                Runtime Dynamic Energy = 1.21024e-09 J
                Total Runtime Energy = 1.72368e-09 J

              Store Queue:
                Area = 0.0608565 mm^2
                Peak Dynamic Power = 0.0421944 W
                Subthreshold Leakage Power = 0.00815046 W
                Gate Leakage Power = 0.000297452 W
                Runtime Dynamic Power = 0.0365685 W
                Runtime Dynamic Energy = 3.22663e-09 J
                Total Runtime Energy = 3.97204e-09 J

          Memory Management Unit:
            Area = 0.331371 mm^2
            Peak Dynamic Power = 0.318513 W
            Subthreshold Leakage Power = 0.097099 W
            Gate Leakage Power = 0.00441089 W
            Runtime Dynamic Power = 0.123948 W
            Runtime Dynamic Energy = 1.09366e-08 J
            Total Runtime Energy = 1.98933e-08 J

              Instruction TLB:
                Area = 0.131789 mm^2
                Peak Dynamic Power = 0.151159 W
                Subthreshold Leakage Power = 0.0446376 W
                Gate Leakage Power = 0.00203139 W
                Runtime Dynamic Power = 0.0511229 W
                Runtime Dynamic Energy = 4.51085e-09 J
                Total Runtime Energy = 8.62869e-09 J

              Data TLB:
                Area = 0.199582 mm^2
                Peak Dynamic Power = 0.167354 W
                Subthreshold Leakage Power = 0.0524614 W
                Gate Leakage Power = 0.00237949 W
                Runtime Dynamic Power = 0.072825 W
                Runtime Dynamic Energy = 6.42574e-09 J
                Total Runtime Energy = 1.12646e-08 J

          Execution Unit:
            Area = 2.36584 mm^2
            Peak Dynamic Power = 1.52633 W
            Subthreshold Leakage Power = 1.18035 W
            Gate Leakage Power = 0.0498689 W
            Runtime Dynamic Power = 0.517033 W
            Runtime Dynamic Energy = 4.56205e-08 J
            Total Runtime Energy = 1.5417e-07 J

              Int Bypass Data:
                Area = 0.0024813 mm^2
                Peak Dynamic Power = 0 W
                Subthreshold Leakage Power = 0 W
                Gate Leakage Power = 0 W
                Runtime Dynamic Power = 0.00618474 W
                Runtime Dynamic Energy = 5.45712e-10 J
                Total Runtime Energy = 5.45712e-10 J

              Int Bypass Tag:
                Area = 0.000291384 mm^2
                Peak Dynamic Power = 0 W
                Subthreshold Leakage Power = 0 W
                Gate Leakage Power = 0 W
                Runtime Dynamic Power = 0.000726287 W
                Runtime Dynamic Energy = 6.40842e-11 J
                Total Runtime Energy = 6.40842e-11 J

              Mul Bypass Data:
                Area = 0.00328459 mm^2
                Peak Dynamic Power = 0 W
                Subthreshold Leakage Power = 0 W
                Gate Leakage Power = 0 W
                Runtime Dynamic Power = 0.00818697 W
                Runtime Dynamic Energy = 7.2238e-10 J
                Total Runtime Energy = 7.2238e-10 J

              Mul Bypass Tag:
                Area = 0.000366693 mm^2
                Peak Dynamic Power = 0 W
                Subthreshold Leakage Power = 0 W
                Gate Leakage Power = 0 W
                Runtime Dynamic Power = 0.000913997 W
                Runtime Dynamic Energy = 8.06468e-11 J
                Total Runtime Energy = 8.06468e-11 J

              FP Bypass Data:
                Area = 0.0039374 mm^2
                Peak Dynamic Power = 0 W
                Subthreshold Leakage Power = 0 W
                Gate Leakage Power = 0 W
                Runtime Dynamic Power = 0.00981414 W
                Runtime Dynamic Energy = 8.65954e-10 J
                Total Runtime Energy = 8.65954e-10 J

              FP Bypass Tag:
                Area = 0.000508858 mm^2
                Peak Dynamic Power = 0 W
                Subthreshold Leakage Power = 0 W
                Gate Leakage Power = 0 W
                Runtime Dynamic Power = 0.00126835 W
                Runtime Dynamic Energy = 1.11913e-10 J
                Total Runtime Energy = 1.11913e-10 J

              Register File Unit:
                Area = 0.0603417 mm^2
                Peak Dynamic Power = 0.094149 W
                Subthreshold Leakage Power = 0.00361325 W
                Gate Leakage Power = 0.000100838 W
                Runtime Dynamic Power = 0.00713589 W
                Runtime Dynamic Energy = 6.29638e-10 J
                Total Runtime Energy = 9.57351e-10 J

                  Integer Register File:
                    Area = 0.0397387 mm^2
                    Peak Dynamic Power = 0.0858804 W
                    Subthreshold Leakage Power = 0.00167327 W
                    Gate Leakage Power = 4.73072e-05 W
                    Runtime Dynamic Power = 0.00340795 W
                    Runtime Dynamic Energy = 3.00702e-10 J
                    Total Runtime Energy = 4.52517e-10 J

                  FP Register File:
                    Area = 0.020603 mm^2
                    Peak Dynamic Power = 0.00826856 W
                    Subthreshold Leakage Power = 0.00193998 W
                    Gate Leakage Power = 5.35312e-05 W
                    Runtime Dynamic Power = 0.00372794 W
                    Runtime Dynamic Energy = 3.28936e-10 J
                    Total Runtime Energy = 5.04834e-10 J

              Instruction Scheduler:
                Area = 0.107117 mm^2
                Peak Dynamic Power = 0.107009 W
                Subthreshold Leakage Power = 0.00250283 W
                Gate Leakage Power = 7.07223e-05 W
                Runtime Dynamic Power = 0.0155966 W
                Runtime Dynamic Energy = 1.37617e-09 J
                Total Runtime Energy = 1.60325e-09 J

                  Integer Instruction Window:
                    Area = 0.0261741 mm^2
                    Peak Dynamic Power = 0.0268581 W
                    Subthreshold Leakage Power = 0 W
                    Gate Leakage Power = 0 W
                    Runtime Dynamic Power = 0.00223817 W
                    Runtime Dynamic Energy = 1.97486e-10 J
                    Total Runtime Energy = 1.97486e-10 J

                  FP Instruction Window:
                    Area = 0.0232716 mm^2
                    Peak Dynamic Power = 0.0133785 W
                    Subthreshold Leakage Power = 0 W
                    Gate Leakage Power = 0 W
                    Runtime Dynamic Power = 0.00222975 W
                    Runtime Dynamic Energy = 1.96742e-10 J
                    Total Runtime Energy = 1.96742e-10 J

                  Reorder Buffer:
                    Area = 0.0576711 mm^2
                    Peak Dynamic Power = 0.066772 W
                    Subthreshold Leakage Power = 0.00250283 W
                    Gate Leakage Power = 7.07223e-05 W
                    Runtime Dynamic Power = 0.0111287 W
                    Runtime Dynamic Energy = 9.81941e-10 J
                    Total Runtime Energy = 1.20902e-09 J

              Integer ALU(s):
                Area = 0.138846 mm^2
                Peak Dynamic Power = 0.332578 W
                Subthreshold Leakage Power = 0.201977 W
                Gate Leakage Power = 0.00854828 W
                Runtime Dynamic Power = 0.0778676 W
                Runtime Dynamic Energy = 6.87067e-09 J
                Total Runtime Energy = 2.54464e-08 J

              Floating Point Unit(s):
                Area = 1.8404 mm^2
                Peak Dynamic Power = 0.595559 W
                Subthreshold Leakage Power = 0.669296 W
                Gate Leakage Power = 0.0283266 W
                Runtime Dynamic Power = 0.233603 W
                Runtime Dynamic Energy = 2.0612e-08 J
                Total Runtime Energy = 8.21669e-08 J

              Multiply/Divide Unit(s):
                Area = 0.20827 mm^2
                Peak Dynamic Power = 0.39704 W
                Subthreshold Leakage Power = 0.302965 W
                Gate Leakage Power = 0.0128224 W
                Runtime Dynamic Power = 0.155735 W
                Runtime Dynamic Energy = 1.37413e-08 J
                Total Runtime Energy = 4.1605e-08 J

          Undifferentiated Core:
            Area = 3.88668 mm^2
            Peak Dynamic Power = 0 W
            Subthreshold Leakage Power = 2.82694 W
            Gate Leakage Power = 0.119645 W
            Runtime Dynamic Power = 0 W
            Runtime Dynamic Energy = 0 J
            Total Runtime Energy = 2.59992e-07 J

          Rename Unit:
            Area = 0.333151 mm^2
            Peak Dynamic Power = 0.10888 W
            Subthreshold Leakage Power = 0.0255114 W
            Gate Leakage Power = 0.000663381 W
            Runtime Dynamic Power = 0.0538848 W
            Runtime Dynamic Energy = 4.75454e-09 J
            Total Runtime Energy = 7.06408e-09 J

              Int Front RAT:
                Area = 0.129348 mm^2
                Peak Dynamic Power = 0.0382386 W
                Subthreshold Leakage Power = 0.00828989 W
                Gate Leakage Power = 0.000204367 W
                Runtime Dynamic Power = 0.0063731 W
                Runtime Dynamic Energy = 5.62332e-10 J
                Total Runtime Energy = 1.31183e-09 J

              FP Front RAT:
                Area = 0.166163 mm^2
                Peak Dynamic Power = 0.0432953 W
                Subthreshold Leakage Power = 0.0126995 W
                Gate Leakage Power = 0.000319816 W
                Runtime Dynamic Power = 0.00721588 W
                Runtime Dynamic Energy = 6.36696e-10 J
                Total Runtime Energy = 1.78546e-09 J

              Integer Free List:
                Area = 0.0120305 mm^2
                Peak Dynamic Power = 0.00394808 W
                Subthreshold Leakage Power = 0.000639181 W
                Gate Leakage Power = 2.0232e-05 W
                Runtime Dynamic Power = 0.00131603 W
                Runtime Dynamic Energy = 1.1612e-10 J
                Total Runtime Energy = 1.74304e-10 J

              Int Retire RAT:
                Area = 0.00606308 mm^2
                Peak Dynamic Power = 0.00325948 W
                Subthreshold Leakage Power = 0.000496413 W
                Gate Leakage Power = 1.45535e-05 W
                Runtime Dynamic Power = 0.000543246 W
                Runtime Dynamic Energy = 4.79335e-11 J
                Total Runtime Energy = 9.30188e-11 J

              FP Retire RAT:
                Area = 0.00751656 mm^2
                Peak Dynamic Power = 0.00404193 W
                Subthreshold Leakage Power = 0.000709488 W
                Gate Leakage Power = 1.94961e-05 W
                Runtime Dynamic Power = 0.000673654 W
                Runtime Dynamic Energy = 5.94401e-11 J
                Total Runtime Energy = 1.23762e-10 J

              FP Free List:
                Area = 0.0120305 mm^2
                Peak Dynamic Power = 0.00394808 W
                Subthreshold Leakage Power = 0.000639181 W
                Gate Leakage Power = 2.0232e-05 W
                Runtime Dynamic Power = 0.00131603 W
                Runtime Dynamic Energy = 1.1612e-10 J
                Total Runtime Energy = 1.74304e-10 J

              Instruction Dependency Check?:
                Area = 0 mm^2
                Peak Dynamic Power = 0.00607447 W
                Subthreshold Leakage Power = 0.00101891 W
                Gate Leakage Power = 3.23427e-05 W
                Runtime Dynamic Power = 0.0242979 W
                Runtime Dynamic Energy = 2.14393e-09 J
                Total Runtime Energy = 2.23669e-09 J

              FP Dependency Check?:
                Area = 0 mm^2
                Peak Dynamic Power = 0.00607447 W
                Subthreshold Leakage Power = 0.00101891 W
                Gate Leakage Power = 3.23427e-05 W
                Runtime Dynamic Power = 0.0121489 W
                Runtime Dynamic Energy = 1.07197e-09 J
                Total Runtime Energy = 1.16472e-09 J

          Pipeline?:
            Area = 0.0912321 mm^2
            Peak Dynamic Power = 0 W
            Subthreshold Leakage Power = 0.0748063 W
            Gate Leakage Power = 0.00796757 W
            Runtime Dynamic Power = 0.269895 W
            Runtime Dynamic Energy = 2.38143e-08 J
            Total Runtime Energy = 3.11178e-08 J

