McPAT (version 0.8 of Aug, 2010) is computing the target processor...
 
Warning: Branch Target Buffer array structure cannot satisfy latency constraint.

McPAT (version 0.8 of Aug, 2010) results  (current print level is 5)
*****************************************************************************************
  Technology 40 nm
  Using Long Channel Devices When Appropriate
  Interconnect metal projection= conservative interconnect technology projection
  Core clock Rate(MHz) 2000

*****************************************************************************************
Processor: 
  Area = 5.83937 mm^2
  Peak Power = 1.32283 W
  Total Leakage = 0.182558 W
  Peak Dynamic = 1.14027 W
  Subthreshold Leakage = 0.0869601 W
  Gate Leakage = 0.095598 W
  Runtime Dynamic = 2.86361 W

  Total Cores: 
  Device Type= ITRS low operating power device type
    Area = 5.33485 mm^2
    Peak Dynamic = 1.07823 W
    Subthreshold Leakage = 0.0827641 W
    Gate Leakage = 0.0887315 W
    Runtime Dynamic = 0.975395 W

  Total First Level Directory: 
  Device Type= ITRS low operating power device type
    Area = 0.489711 mm^2
    Peak Dynamic = 0.0449752 W
    Subthreshold Leakage = 0.00397708 W
    Gate Leakage = 0.00655632 W
    Runtime Dynamic = 1.80289 W

  Total NoCs (Network/Bus): 
  Device Type= ITRS low operating power device type
    Area = 0.0148119 mm^2
    Peak Dynamic = 0.0170648 W
    Subthreshold Leakage = 0.000218992 W
    Gate Leakage = 0.000310207 W
    Runtime Dynamic = 0.0853239 W

*****************************************************************************************
Core:
      Area = 2.66742 mm^2
      Peak Dynamic = 0.539116 W
      Subthreshold Leakage = 0.041382 W
      Gate Leakage = 0.0443657 W
      Runtime Dynamic = 0.975395 W

      Instruction Fetch Unit:
        Area = 0.565848 mm^2
        Peak Dynamic = 0.184724 W
        Subthreshold Leakage = 0.00572394 W
        Gate Leakage = 0.00380598 W
        Runtime Dynamic = 0.283222 W

          Instruction Cache:
            Area = 0.235613 mm^2
            Peak Dynamic = 0.0310428 W
            Subthreshold Leakage = 0.00309635 W
            Gate Leakage = 0.00216385 W
            Runtime Dynamic = 0.0461626 W

          Branch Target Buffer:
            Area = 0.251259 mm^2
            Peak Dynamic = 0.0174433 W
            Subthreshold Leakage = 0.00170231 W
            Gate Leakage = 0.000908123 W
            Runtime Dynamic = 0.0697733 W

          Branch Predictor:
            Area = 0.064441 mm^2
            Peak Dynamic = 0.00815792 W
            Subthreshold Leakage = 0.00070444 W
            Gate Leakage = 0.000477387 W
            Runtime Dynamic = 0.0113878 W

              Global Predictor:
                Area = 0.0313969 mm^2
                Peak Dynamic = 0.00374527 W
                Subthreshold Leakage = 0.00034631 W
                Gate Leakage = 0.000233555 W
                Runtime Dynamic = 0.00545806 W

              Local Predictor:
                Area = 0.000711939 mm^2
                Peak Dynamic = 0.000301014 W
                Subthreshold Leakage = 6.13457e-06 W
                Gate Leakage = 5.63471e-06 W
                Runtime Dynamic = 0.000471566 W

                Area = 0.000650815 mm^2
                Peak Dynamic = 0.000230123 W
                Subthreshold Leakage = 5.7769e-06 W
                Gate Leakage = 4.75075e-06 W
                Runtime Dynamic = 0.000354988 W

              Chooser:
                Area = 0.0313969 mm^2
                Peak Dynamic = 0.00374527 W
                Subthreshold Leakage = 0.00034631 W
                Gate Leakage = 0.000233555 W
                Runtime Dynamic = 0.00545806 W

              RAS:
                Area = 0.000996272 mm^2
                Peak Dynamic = 0.000366372 W
                Subthreshold Leakage = 5.68653e-06 W
                Gate Leakage = 4.64147e-06 W
                Runtime Dynamic = 6.23994e-08 W

          Instruction Buffer:
            Area = 0.00820192 mm^2
            Peak Dynamic = 0.0669878 W
            Subthreshold Leakage = 6.33536e-05 W
            Gate Leakage = 4.34841e-05 W
            Runtime Dynamic = 0.0382787 W

          Instruction Decoder:
            Area = 0.00468731 mm^2
            Peak Dynamic = 0.05881 W
            Subthreshold Leakage = 0.000127696 W
            Gate Leakage = 0.000115494 W
            Runtime Dynamic = 0.11762 W

      Renaming Unit:
        Area = 0.0903068 mm^2
        Peak Dynamic = 0.0451514 W
        Subthreshold Leakage = 0.000345688 W
        Gate Leakage = 0.00032022 W
        Runtime Dynamic = 0.0731287 W

          Int Front End RAT:
            Area = 0.0543672 mm^2
            Peak Dynamic = 0.0237617 W
            Subthreshold Leakage = 0.000175223 W
            Gate Leakage = 0.000121525 W
            Runtime Dynamic = 0.0475234 W

          FP Front End RAT:
            Area = 0.0185325 mm^2
            Peak Dynamic = 0.00949419 W
            Subthreshold Leakage = 0.000100325 W
            Gate Leakage = 6.76251e-05 W
            Runtime Dynamic = 0.00949419 W

          Free List:
            Area = 0.00599955 mm^2
            Peak Dynamic = 0.00225065 W
            Subthreshold Leakage = 1.24363e-05 W
            Gate Leakage = 1.00844e-05 W
            Runtime Dynamic = 0.0090026 W

          Int Retire RAT: 
            Area = 0.00605969 mm^2
            Peak Dynamic = 0.00448392 W
            Subthreshold Leakage = 1.33231e-05 W
            Gate Leakage = 1.16235e-05 W
            Runtime Dynamic = 0.00448392 W

          FP Retire RAT:
            Area = 0.000650815 mm^2
            Peak Dynamic = 0.00067334 W
            Subthreshold Leakage = 5.7769e-06 W
            Gate Leakage = 4.75075e-06 W
            Runtime Dynamic = 0.00067334 W

          FP Free List:
            Area = 0.00305098 mm^2
            Peak Dynamic = 0.00195124 W
            Subthreshold Leakage = 8.81712e-06 W
            Gate Leakage = 6.96054e-06 W
            Runtime Dynamic = 0.00195124 W

      Load Store Unit:
        Area = 0.274913 mm^2
        Peak Dynamic = 0.0347482 W
        Subthreshold Leakage = 0.0032012 W
        Gate Leakage = 0.00235752 W
        Runtime Dynamic = 0.195304 W

          Data Cache:
            Area = 0.240878 mm^2
            Peak Dynamic = 0.0293665 W
            Subthreshold Leakage = 0.00312878 W
            Gate Leakage = 0.00220794 W
            Runtime Dynamic = 0.19026 W

          StoreQ:
            Area = 0.00754674 mm^2
            Peak Dynamic = 0.00358087 W
            Subthreshold Leakage = 4.2633e-05 W
            Gate Leakage = 5.19212e-05 W
            Runtime Dynamic = 0.00504348 W

      Memory Management Unit:
        Area = 0.021508 mm^2
        Peak Dynamic = 0.0127337 W
        Subthreshold Leakage = 0.000210621 W
        Gate Leakage = 0.000290666 W
        Runtime Dynamic = 0.037071 W

          Itlb:
            Area = 0.00993091 mm^2
            Peak Dynamic = 0.00617846 W
            Subthreshold Leakage = 9.04168e-05 W
            Gate Leakage = 9.65082e-05 W
            Runtime Dynamic = 0.012357 W

          Dtlb:
            Area = 0.00993091 mm^2
            Peak Dynamic = 0.00438671 W
            Subthreshold Leakage = 9.04168e-05 W
            Gate Leakage = 9.65082e-05 W
            Runtime Dynamic = 0.0247139 W

      Execution Unit:
        Area = 1.65498 mm^2
        Peak Dynamic = 0.261758 W
        Subthreshold Leakage = 0.0305522 W
        Gate Leakage = 0.0360036 W
        Runtime Dynamic = 0.386669 W

          Register Files:
            Area = 0.203203 mm^2
            Peak Dynamic = 0.0763282 W
            Subthreshold Leakage = 0.000197046 W
            Gate Leakage = 0.00016338 W
            Runtime Dynamic = 0.0386066 W

              Integer RF:
                Area = 0.146073 mm^2
                Peak Dynamic = 0.0763282 W
                Subthreshold Leakage = 0.000120303 W
                Gate Leakage = 9.97867e-05 W
                Runtime Dynamic = 0.0345689 W

              Floating Point RF:
                Area = 0.05713 mm^2
                Peak Dynamic = 0 W
                Subthreshold Leakage = 7.67427e-05 W
                Gate Leakage = 6.35938e-05 W
                Runtime Dynamic = 0.00403765 W

          Instruction Scheduler:
            Area = 0.0582889 mm^2
            Peak Dynamic = 0.0522571 W
            Subthreshold Leakage = 0.000128698 W
            Gate Leakage = 0.000185714 W
            Runtime Dynamic = 0.0787473 W

              Instruction Window:
                Area = 0.053925 mm^2
                Peak Dynamic = 0.0445895 W
                Subthreshold Leakage = 9.52936e-05 W
                Gate Leakage = 0.000130718 W
                Runtime Dynamic = 0.0602231 W

              FP Instruction Window:
                Area = 0.00436388 mm^2
                Peak Dynamic = 0.00766759 W
                Subthreshold Leakage = 3.34043e-05 W
                Gate Leakage = 5.49962e-05 W
                Runtime Dynamic = 0.0185242 W

          Integer ALUs (Count: 3 ):
            Area = 0.312404 mm^2
            Peak Dynamic = 0.0283684 W
            Subthreshold Leakage = 0.0140724 W
            Gate Leakage = 0.0165703 W
            Runtime Dynamic = 0.0373268 W

          Floating Point Units (FPUs) (Count: 1 ):
            Area = 0.971259 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0.0109377 W
            Gate Leakage = 0.0128792 W
            Runtime Dynamic = 0.0373268 W

          Complex ALUs (Mul/Div) (Count: 1 ):
            Area = 0.104135 mm^2
            Peak Dynamic = 0.0204053 W
            Subthreshold Leakage = 0.00469079 W
            Gate Leakage = 0.00552345 W
            Runtime Dynamic = 0.049769 W

          Results Broadcast Bus:
            Area Overhead = 0.00404385 mm^2
            Peak Dynamic = 0.0824719 W
            Subthreshold Leakage = 0.000495836 W
            Gate Leakage = 0.000583852 W
            Runtime Dynamic = 0.144892 W

*****************************************************************************************
First Level Directory
      Area = 0.244856 mm^2
      Peak Dynamic = 0.0224876 W
      Subthreshold Leakage = 0.00198854 W
      Gate Leakage = 0.00327816 W
      Runtime Dynamic = 1.80289 W

*****************************************************************************************
BUSES
      Area = 0.0148119 mm^2
      Peak Dynamic = 0.0170648 W
      Subthreshold Leakage = 0.000218992 W
      Gate Leakage = 0.000310207 W
      Runtime Dynamic = 0.0853239 W

      Bus: 
        Area = 0.0148119 mm^2
        Peak Dynamic = 0.0170648 W
        Subthreshold Leakage = 0.000218992 W
        Gate Leakage = 0.000310207 W
        Runtime Dynamic = 0.0853239 W

*****************************************************************************************
