McPAT (version 0.8 of Aug, 2010) is computing the target processor...
 
line64
size1.04858e+06
line9
size8.38861e+06

McPAT (version 0.8 of Aug, 2010) results  (current print level is 5)
*****************************************************************************************
  Technology 22 nm
  Using Long Channel Devices When Appropriate
  Interconnect metal projection= aggressive interconnect technology projection
  Core clock Rate(MHz) 3500

*****************************************************************************************
Processor: 
  Area = 358.016 mm^2
  Peak Power = 168.519 W
  Total Leakage = 30.8855 W
  Peak Dynamic = 137.634 W
  Subthreshold Leakage = 30.5351 W
  Gate Leakage = 0.350385 W
  Runtime Dynamic = 84.2366 W

  Total Cores: 64 cores 
  Device Type= ITRS high performance device type
    Area = 87.1986 mm^2
    Peak Dynamic = 42.426 W
    Subthreshold Leakage = 7.80232 W
    Gate Leakage = 0.0799149 W
    Runtime Dynamic = 9.61388 W

  Total L2s: 
  Device Type= ITRS high performance device type
    Area = 161.532 mm^2
    Peak Dynamic = 21.1059 W
    Subthreshold Leakage = 8.9583 W
    Gate Leakage = 0.100733 W
    Runtime Dynamic = 1.14063 W

  Total First Level Directory: 
  Device Type= ITRS high performance device type
    Area = 57.033 mm^2
    Peak Dynamic = 53.5219 W
    Subthreshold Leakage = 4.27249 W
    Gate Leakage = 0.050206 W
    Runtime Dynamic = 70.9203 W

  Total NoCs (Network/Bus): 
  Device Type= ITRS high performance device type
    Area = 52.2524 mm^2
    Peak Dynamic = 20.5798 W
    Subthreshold Leakage = 9.50197 W
    Gate Leakage = 0.119531 W
    Runtime Dynamic = 2.56185 W

*****************************************************************************************
Core:
      Area = 1.36248 mm^2
      Peak Dynamic = 0.662906 W
      Subthreshold Leakage = 0.121911 W
      Gate Leakage = 0.00124867 W
      Runtime Dynamic = 9.61388 W

      Instruction Fetch Unit:
        Area = 0.140786 mm^2
        Peak Dynamic = 0.0863256 W
        Subthreshold Leakage = 0.00636762 W
        Gate Leakage = 7.4998e-05 W
        Runtime Dynamic = 2.08883 W

          Instruction Cache:
            Area = 0.129377 mm^2
            Peak Dynamic = 0.0476007 W
            Subthreshold Leakage = 0.00381804 W
            Gate Leakage = 2.35266e-05 W
            Runtime Dynamic = 0.0698158 W

          Instruction Buffer:
            Area = 0.000754971 mm^2
            Peak Dynamic = 0.00238165 W
            Subthreshold Leakage = 4.99334e-05 W
            Gate Leakage = 3.27157e-07 W
            Runtime Dynamic = 0.0190532 W

          Instruction Decoder:
            Area = 0.00131543 mm^2
            Peak Dynamic = 0.0246042 W
            Subthreshold Leakage = 0.000538954 W
            Gate Leakage = 3.91915e-06 W
            Runtime Dynamic = 0.196833 W

      Load Store Unit:
        Area = 0.0977414 mm^2
        Peak Dynamic = 0.0587123 W
        Subthreshold Leakage = 0.00580883 W
        Gate Leakage = 7.48788e-05 W
        Runtime Dynamic = 2.07447 W

          Data Cache:
            Area = 0.0569223 mm^2
            Peak Dynamic = 0.0329939 W
            Subthreshold Leakage = 0.00249221 W
            Gate Leakage = 1.63814e-05 W
            Runtime Dynamic = 0.0476753 W

          Load/Store Queue:
            Area = 0.023444 mm^2
            Peak Dynamic = 0.0139792 W
            Subthreshold Leakage = 0.00135593 W
            Gate Leakage = 1.12722e-05 W
            Runtime Dynamic = 0.223667 W

      Memory Management Unit:
        Area = 0.0313997 mm^2
        Peak Dynamic = 0.0446647 W
        Subthreshold Leakage = 0.0029577 W
        Gate Leakage = 5.57335e-05 W
        Runtime Dynamic = 1.92566 W

          Itlb:
            Area = 0.0110306 mm^2
            Peak Dynamic = 0.0122535 W
            Subthreshold Leakage = 0.000498504 W
            Gate Leakage = 4.25417e-06 W
            Runtime Dynamic = 0.0980282 W

          Dtlb:
            Area = 0.0110306 mm^2
            Peak Dynamic = 0.00306337 W
            Subthreshold Leakage = 0.000498504 W
            Gate Leakage = 4.25417e-06 W
            Runtime Dynamic = 0.0245072 W

      Execution Unit:
        Area = 0.299667 mm^2
        Peak Dynamic = 0.473204 W
        Subthreshold Leakage = 0.0379242 W
        Gate Leakage = 0.000384077 W
        Runtime Dynamic = 3.52491 W

          Register Files:
            Area = 0.0598365 mm^2
            Peak Dynamic = 0.0168768 W
            Subthreshold Leakage = 0.0020814 W
            Gate Leakage = 1.24237e-05 W
            Runtime Dynamic = 0.072481 W

              Integer RF:
                Area = 0.0240072 mm^2
                Peak Dynamic = 0.0131657 W
                Subthreshold Leakage = 0.000449165 W
                Gate Leakage = 3.33111e-06 W
                Runtime Dynamic = 0.0706931 W

              Floating Point RF:
                Area = 0.0240072 mm^2
                Peak Dynamic = 0.00371113 W
                Subthreshold Leakage = 0.000449165 W
                Gate Leakage = 3.33111e-06 W
                Runtime Dynamic = 0.0017722 W

              Register Windows:
                Area = 0.0118221 mm^2
                Peak Dynamic = 0 W
                Subthreshold Leakage = 0.00118307 W
                Gate Leakage = 5.76149e-06 W
                Runtime Dynamic = 1.56951e-05 W

          Instruction Scheduler:
            Area = 0.00263062 mm^2
            Peak Dynamic = 0.00540689 W
            Subthreshold Leakage = 8.27524e-05 W
            Gate Leakage = 9.38261e-07 W
            Runtime Dynamic = 0.0464411 W

              Instruction Window:
                Area = 0.00263062 mm^2
                Peak Dynamic = 0.00540689 W
                Subthreshold Leakage = 8.27524e-05 W
                Gate Leakage = 9.38261e-07 W
                Runtime Dynamic = 0.0464411 W

          Integer ALUs (Count: 1 ):
            Area = 0.0384544 mm^2
            Peak Dynamic = 0.0946992 W
            Subthreshold Leakage = 0.00667865 W
            Gate Leakage = 6.39207e-05 W
            Runtime Dynamic = 0.841771 W

          Floating Point Units (FPUs) (Count: 0.125 ):
            Area = 0.0695899 mm^2
            Peak Dynamic = 0.0157832 W
            Subthreshold Leakage = 0.00302155 W
            Gate Leakage = 2.89189e-05 W
            Runtime Dynamic = 0.0315664 W

          Complex ALUs (Mul/Div) (Count: 1 ):
            Area = 0.115363 mm^2
            Peak Dynamic = 0.105221 W
            Subthreshold Leakage = 0.020036 W
            Gate Leakage = 0.000191762 W
            Runtime Dynamic = 0.210443 W

          Results Broadcast Bus:
            Area Overhead = 0.00445381 mm^2
            Peak Dynamic = 0.192955 W
            Subthreshold Leakage = 0.00406321 W
            Gate Leakage = 3.88886e-05 W
            Runtime Dynamic = 0.519078 W

*****************************************************************************************
L2
      Area = 2.52394 mm^2
      Peak Dynamic = 0.32978 W
      Subthreshold Leakage = 0.139973 W
      Gate Leakage = 0.00157395 W
      Runtime Dynamic = 1.14063 W

*****************************************************************************************
Second Level Directory
      Area = 57.033 mm^2
      Peak Dynamic = 53.5219 W
      Subthreshold Leakage = 4.27249 W
      Gate Leakage = 0.050206 W
      Runtime Dynamic = 70.9203 W

*****************************************************************************************
NOC
      Area = 52.2524 mm^2
      Peak Dynamic = 20.5798 W
      Subthreshold Leakage = 9.50197 W
      Gate Leakage = 0.119531 W
      Runtime Dynamic = 2.56185 W

      Router: 
        Area = 0.578434 mm^2
        Peak Dynamic = 0.184548 W
        Subthreshold Leakage = 0.125515 W
        Gate Leakage = 0.0016409 W
        Runtime Dynamic = 1.32875 W

            Virtual Channel Buffer:
              Area = 0.159162 mm^2
              Peak Dynamic = 0.00394081 W
              Subthreshold Leakage = 0.000194478 W
              Gate Leakage = 1.84946e-06 W
              Runtime Dynamic = 0.0283738 W

            Crossbar:
              Area = 0.160976 mm^2
              Peak Dynamic = 0.179891 W
              Subthreshold Leakage = 0.12532 W
              Gate Leakage = 0.00163905 W
              Runtime Dynamic = 1.29522 W

            Arbiter:
              Peak Dynamic = 0.000716053 W
              Subthreshold Leakage = 3.67148e-07 W
              Gate Leakage = 3.86991e-09 W
              Runtime Dynamic = 0.00515558 W

      Per Router Links: 
        Area = 0.238009 mm^2
        Peak Dynamic = 0.137011 W
        Subthreshold Leakage = 0.0229533 W
        Gate Leakage = 0.000226773 W
        Runtime Dynamic = 1.2331 W

*****************************************************************************************
