
/*
 * Copyright (c) 1999-2005 Mark D. Hill and David A. Wood
 * All rights reserved.
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions are
 * met: redistributions of source code must retain the above copyright
 * notice, this list of conditions and the following disclaimer;
 * redistributions in binary form must reproduce the above copyright
 * notice, this list of conditions and the following disclaimer in the
 * documentation and/or other materials provided with the distribution;
 * neither the name of the copyright holders nor the names of its
 * contributors may be used to endorse or promote products derived from
 * this software without specific prior written permission.
 *
 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
 * "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
 * LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
 * A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
 * OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
 * SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
 * LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
 * DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
 * THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
 * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

/*
 * $Id$
 *
 */

// MemoryRequestType used in MemoryMsg

enumeration(MemoryRequestType, desc="...") {

  // Southbound request: from directory to memory cache
  // or directory to memory or memory cache to memory
  MEMORY_READ,     desc="Read request to memory";
  MEMORY_WB,       desc="Write back data to memory";

  // response from memory to directory
  // (These are currently unused!)
  MEMORY_DATA, desc="Data read from memory";
  MEMORY_ACK,  desc="Write to memory acknowledgement";
}


// Message to and from Memory Control

structure(MemoryMsg, desc="...", interface="Message") {
  Address Addr,              desc="Physical address for this request";
  MemoryRequestType Type,       desc="Type of memory request (MEMORY_READ or MEMORY_WB)";
  MachineID Sender,             desc="What component sent the data";
  MachineID OriginalRequestorMachId, desc="What component originally requested";
  DataBlock DataBlk,            desc="Data to writeback";
  MessageSizeType MessageSize,  desc="size category of the message";
  // Not all fields used by all protocols:
  PrefetchBit Prefetch,         desc="Is this a prefetch request";
  bool ReadX,                   desc="Exclusive";
  int Acks,                     desc="How many acks to expect";

  bool functionalRead(Packet *pkt) {
    return testAndRead(Addr, DataBlk, pkt);
  }

  bool functionalWrite(Packet *pkt) {
    return testAndWrite(Addr, DataBlk, pkt);
  }
}
