/*
 * Copyright (c) 2012-2015 Advanced Micro Devices, Inc.
 * All rights reserved.
 *
 * For use for simulation and test purposes only
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions are met:
 *
 * 1. Redistributions of source code must retain the above copyright notice,
 * this list of conditions and the following disclaimer.
 *
 * 2. Redistributions in binary form must reproduce the above copyright notice,
 * this list of conditions and the following disclaimer in the documentation
 * and/or other materials provided with the distribution.
 *
 * 3. Neither the name of the copyright holder nor the names of its contributors
 * may be used to endorse or promote products derived from this software
 * without specific prior written permission.
 *
 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
 * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
 * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
 * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE
 * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
 * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
 * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
 * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
 * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
 * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
 * POSSIBILITY OF SUCH DAMAGE.
 *
 * Author: Blake Hechtman
 */

machine(MachineType:SQC, "GPU SQC (L1 I Cache)")
 : Sequencer* sequencer;
   CacheMemory * L1cache;
   int TCC_select_num_bits;
   Cycles issue_latency := 80;  // time to send data down to TCC
   Cycles l2_hit_latency := 18; // for 1MB L2, 20 for 2MB

  MessageBuffer * requestFromSQC, network="To", virtual_network="1", vnet_type="request";

  MessageBuffer * probeToSQC, network="From", virtual_network="1", vnet_type="request";
  MessageBuffer * responseToSQC, network="From", virtual_network="3", vnet_type="response";

  MessageBuffer * mandatoryQueue;
{
  state_declaration(State, desc="SQC Cache States", default="SQC_State_I") {
    I, AccessPermission:Invalid, desc="Invalid";
    V, AccessPermission:Read_Only, desc="Valid";
  }

  enumeration(Event, desc="SQC Events") {
    // Core initiated
    Fetch,          desc="Fetch";
    // Mem sys initiated
    Repl,           desc="Replacing block from cache";
    Data,           desc="Received Data";
  }

  enumeration(RequestType, desc="To communicate stats from transitions to recordStats") {
    DataArrayRead,    desc="Read the data array";
    DataArrayWrite,   desc="Write the data array";
    TagArrayRead,     desc="Read the data array";
    TagArrayWrite,    desc="Write the data array";
  }


  structure(Entry, desc="...", interface="AbstractCacheEntry") {
    State CacheState,           desc="cache state";
    bool Dirty,                 desc="Is the data dirty (diff than memory)?";
    DataBlock DataBlk,          desc="data for the block";
    bool FromL2, default="false", desc="block just moved from L2";
  }

  structure(TBE, desc="...") {
    State TBEState,             desc="Transient state";
    DataBlock DataBlk,       desc="data for the block, required for concurrent writebacks";
    bool Dirty,              desc="Is the data dirty (different than memory)?";
    int NumPendingMsgs,      desc="Number of acks/data messages that this processor is waiting for";
    bool Shared,             desc="Victim hit by shared probe";
   }

  structure(TBETable, external="yes") {
    TBE lookup(Addr);
    void allocate(Addr);
    void deallocate(Addr);
    bool isPresent(Addr);
  }

  TBETable TBEs, template="<SQC_TBE>", constructor="m_number_of_TBEs";
  int TCC_select_low_bit, default="RubySystem::getBlockSizeBits()";

  void set_cache_entry(AbstractCacheEntry b);
  void unset_cache_entry();
  void set_tbe(TBE b);
  void unset_tbe();
  void wakeUpAllBuffers();
  void wakeUpBuffers(Addr a);
  Cycles curCycle();

  // Internal functions
  Tick clockEdge();

  Entry getCacheEntry(Addr address), return_by_pointer="yes" {
    Entry cache_entry := static_cast(Entry, "pointer", L1cache.lookup(address));
    return cache_entry;
  }

  DataBlock getDataBlock(Addr addr), return_by_ref="yes" {
    TBE tbe := TBEs.lookup(addr);
    if(is_valid(tbe)) {
      return tbe.DataBlk;
    } else {
      return getCacheEntry(addr).DataBlk;
    }
  }

  State getState(TBE tbe, Entry cache_entry, Addr addr) {
    if(is_valid(tbe)) {
      return tbe.TBEState;
    } else if (is_valid(cache_entry)) {
      return cache_entry.CacheState;
    }
    return State:I;
  }

  void setState(TBE tbe, Entry cache_entry, Addr addr, State state) {
    if (is_valid(tbe)) {
      tbe.TBEState := state;
    }

    if (is_valid(cache_entry)) {
      cache_entry.CacheState := state;
    }
  }

  void functionalRead(Addr addr, Packet *pkt) {
    TBE tbe := TBEs.lookup(addr);
    if(is_valid(tbe)) {
      testAndRead(addr, tbe.DataBlk, pkt);
    } else {
      functionalMemoryRead(pkt);
    }
  }

  int functionalWrite(Addr addr, Packet *pkt) {
    int num_functional_writes := 0;

    TBE tbe := TBEs.lookup(addr);
    if(is_valid(tbe)) {
      num_functional_writes := num_functional_writes +
            testAndWrite(addr, tbe.DataBlk, pkt);
    }

    num_functional_writes := num_functional_writes +
        functionalMemoryWrite(pkt);
    return num_functional_writes;
  }

  AccessPermission getAccessPermission(Addr addr) {
    TBE tbe := TBEs.lookup(addr);
    if(is_valid(tbe)) {
      return SQC_State_to_permission(tbe.TBEState);
    }

    Entry cache_entry := getCacheEntry(addr);
    if(is_valid(cache_entry)) {
      return SQC_State_to_permission(cache_entry.CacheState);
    }

    return AccessPermission:NotPresent;
  }

  void setAccessPermission(Entry cache_entry, Addr addr, State state) {
    if (is_valid(cache_entry)) {
      cache_entry.changePermission(SQC_State_to_permission(state));
    }
  }

  void recordRequestType(RequestType request_type, Addr addr) {
    if (request_type == RequestType:DataArrayRead) {
        L1cache.recordRequestType(CacheRequestType:DataArrayRead, addr);
    } else if (request_type == RequestType:DataArrayWrite) {
        L1cache.recordRequestType(CacheRequestType:DataArrayWrite, addr);
    } else if (request_type == RequestType:TagArrayRead) {
        L1cache.recordRequestType(CacheRequestType:TagArrayRead, addr);
    } else if (request_type == RequestType:TagArrayWrite) {
        L1cache.recordRequestType(CacheRequestType:TagArrayWrite, addr);
    }
  }

  bool checkResourceAvailable(RequestType request_type, Addr addr) {
    if (request_type == RequestType:DataArrayRead) {
      return L1cache.checkResourceAvailable(CacheResourceType:DataArray, addr);
    } else if (request_type == RequestType:DataArrayWrite) {
      return L1cache.checkResourceAvailable(CacheResourceType:DataArray, addr);
    } else if (request_type == RequestType:TagArrayRead) {
      return L1cache.checkResourceAvailable(CacheResourceType:TagArray, addr);
    } else if (request_type == RequestType:TagArrayWrite) {
      return L1cache.checkResourceAvailable(CacheResourceType:TagArray, addr);
    } else {
      error("Invalid RequestType type in checkResourceAvailable");
      return true;
    }
  }

  // Out Ports

  out_port(requestNetwork_out, CPURequestMsg, requestFromSQC);

  // In Ports

  in_port(responseToSQC_in, ResponseMsg, responseToSQC) {
    if (responseToSQC_in.isReady(clockEdge())) {
      peek(responseToSQC_in, ResponseMsg, block_on="addr") {

        Entry cache_entry := getCacheEntry(in_msg.addr);
        TBE tbe := TBEs.lookup(in_msg.addr);

        if (in_msg.Type == CoherenceResponseType:TDSysResp) {
          if (is_valid(cache_entry) || L1cache.cacheAvail(in_msg.addr)) {
            trigger(Event:Data, in_msg.addr, cache_entry, tbe);
          } else {
            Addr victim := L1cache.cacheProbe(in_msg.addr);
            trigger(Event:Repl, victim, getCacheEntry(victim), TBEs.lookup(victim));
          }
        } else {
          error("Unexpected Response Message to Core");
        }
      }
    }
  }

  in_port(mandatoryQueue_in, RubyRequest, mandatoryQueue, desc="...") {
    if (mandatoryQueue_in.isReady(clockEdge())) {
      peek(mandatoryQueue_in, RubyRequest, block_on="LineAddress") {
        Entry cache_entry := getCacheEntry(in_msg.LineAddress);
        TBE tbe := TBEs.lookup(in_msg.LineAddress);

        assert(in_msg.Type == RubyRequestType:IFETCH);
        trigger(Event:Fetch, in_msg.LineAddress, cache_entry, tbe);
      }
    }
  }

  // Actions

  action(ic_invCache, "ic", desc="invalidate cache") {
    if(is_valid(cache_entry)) {
      L1cache.deallocate(address);
    }
    unset_cache_entry();
  }

  action(nS_issueRdBlkS, "nS", desc="Issue RdBlkS") {
    enqueue(requestNetwork_out, CPURequestMsg, issue_latency) {
      out_msg.addr := address;
      out_msg.Type := CoherenceRequestType:RdBlk;
      out_msg.Requestor := machineID;
      out_msg.Destination.add(mapAddressToRange(address,MachineType:TCC,
                              TCC_select_low_bit, TCC_select_num_bits));
      out_msg.MessageSize := MessageSizeType:Request_Control;
      out_msg.InitialRequestTime := curCycle();
    }
  }

  action(a_allocate, "a", desc="allocate block") {
    if (is_invalid(cache_entry)) {
      set_cache_entry(L1cache.allocate(address, new Entry));
    }
  }

  action(p_popMandatoryQueue, "pm", desc="Pop Mandatory Queue") {
    mandatoryQueue_in.dequeue(clockEdge());
  }

  action(pr_popResponseQueue, "pr", desc="Pop Response Queue") {
    responseToSQC_in.dequeue(clockEdge());
  }

  action(l_loadDone, "l", desc="local load done") {
    assert(is_valid(cache_entry));
    sequencer.readCallback(address, cache_entry.DataBlk, false, MachineType:L1Cache);
    APPEND_TRANSITION_COMMENT(cache_entry.DataBlk);
  }

  action(w_writeCache, "w", desc="write data to cache") {
    peek(responseToSQC_in, ResponseMsg) {
      assert(is_valid(cache_entry));
      cache_entry.DataBlk := in_msg.DataBlk;
      cache_entry.Dirty := false;
    }
  }

  // Transitions

  // transitions from base
  transition({I, V}, Repl, I) {TagArrayRead, TagArrayWrite} {
    ic_invCache
  }

  transition(I, Data, V) {TagArrayRead, TagArrayWrite, DataArrayRead} {
    a_allocate;
    w_writeCache
    l_loadDone;
    pr_popResponseQueue;
  }

  transition(I, Fetch) {TagArrayRead, TagArrayWrite} {
    nS_issueRdBlkS;
    p_popMandatoryQueue;
  }

  // simple hit transitions
  transition(V, Fetch) {TagArrayRead, DataArrayRead} {
    l_loadDone;
    p_popMandatoryQueue;
  }
}
