// -*- mode:c++ -*-

// Copyright (c) 2015 RISC-V Foundation
// Copyright (c) 2016 The University of Virginia
// All rights reserved.
//
// Redistribution and use in source and binary forms, with or without
// modification, are permitted provided that the following conditions are
// met: redistributions of source code must retain the above copyright
// notice, this list of conditions and the following disclaimer;
// redistributions in binary form must reproduce the above copyright
// notice, this list of conditions and the following disclaimer in the
// documentation and/or other materials provided with the distribution;
// neither the name of the copyright holders nor the names of its
// contributors may be used to endorse or promote products derived from
// this software without specific prior written permission.
//
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
// "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
// LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
// A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
// OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
// SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
// LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
// DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
// THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
// (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
// OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
//
// Authors: Maxwell Walter
//          Alec Roelke

////////////////////////////////////////////////////////////////////
//
// Bitfield definitions.
//

def bitfield OPCODE <6:0>;
def bitfield NONOPCODE <31:7>;

// R-Type
def bitfield ALL	<31:0>;
def bitfield RD     <11:7>;
def bitfield FUNCT3 <14:12>;
def bitfield RS1    <19:15>;
def bitfield RS2    <24:20>;
def bitfield FUNCT7 <31:25>;

// Bit shifts
def bitfield SRTYPE <30>;
def bitfield SHAMT5 <24:20>;
def bitfield SHAMT6 <25:20>;

// I-Type
def bitfield IMM12  <31:20>;

// S-Type
def bitfield IMM5   <11:7>;
def bitfield IMM7   <31:25>;

// U-Type
def bitfield IMM20  <31:12>;

// SB-Type
def bitfield BIMM12BIT11 <7>;
def bitfield BIMM12BITS4TO1<11:8>;
def bitfield IMMSIGN <31>;
def bitfield BIMM12BITS10TO5 <30:25>;

// UJ-Type
def bitfield UJIMMBITS10TO1 <30:21>;
def bitfield  UJIMMBIT11 <20>;
def bitfield UJIMMBITS19TO12 <19:12>;

// System
def bitfield FUNCT12 <31:20>;
def bitfield ZIMM <19:15>;

// Floating point
def bitfield FD <11:7>;
def bitfield FS1 <19:15>;
def bitfield FS2 <24:20>;
def bitfield FS3 <31:27>;

def bitfield ROUND_MODE <14:12>;
def bitfield CONV_SGN <24:20>;
def bitfield FUNCT2 <26:25>;

// AMO
def bitfield AMOFUNCT <31:27>;
def bitfield AQ <26>;
def bitfield RL <25>;
